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1	ET-SoC-1 Overview
1.1	ET-SoC-1 at a Glance
ET-SoC-1 is a many-core RISC-V system-on-chip developed primarily for artificial-intelligence and machine-learning (AI/ML) workloads. It is designed as a flexible, fast and efficient inference engine for ML applications. Its compute resources are arranged in a multi-level hierarchy that delivers high sustained performance on regular, parallelizable workloads, such as those of ML algorithms.
The device integrates 1,093 general-purpose 64-bit RISC-V cores of three types:
· 1,088 ET-Minion cores for ML computation
· 4 ET-Maxion cores for management and general-purpose tasks
· 1 Service Processor for boot and device management
The cores are connected to on-die SRAM, external memory and a set of standard interfaces through a mesh network-on-chip (NoC). Table 1 summarizes the device.
Table 1. ET-SoC-1 key characteristics
	Item
	Description

	ET-Minion cores
	1,088 in-order, dual-threaded RV64IMFC cores, each with an 8-lane vector/tensor unit

	ET-Maxion cores
	4 single-threaded, superscalar, out-of-order 64-bit RISC-V cores

	Service Processor
	1 single-threaded core derived from the ET-Minion

	On-die SRAM
	Each Minion Shire’s 4 MB Shire Cache can be partitioned by ESRs into L2, a slice of the chip-wide L3, and scratchpad.

	Interconnect
	Mesh NoC with 44 mesh stops

	External memory
	LPDDR4X, 16 channels x 16 bits, up to 4,266 MT/s

	PCI Express
	Gen4, 8 lanes. Endpoint, root complex, or both at once.

	Other interfaces
	eMMC, USB 2.0 OTG, I2C/SMBus, I3C, SPI, UART, GPIO. Debug access through JTAG and a USB 2.0 device port.


1.2	The ET-Minion Hierarchy
The ET-Minion cores are organized in three levels, as shown in Figure 1:
· ET-Minion core
· Neighborhood: 8 ET-Minion cores
· Minion Shire: 4 Neighborhoods (32 ET-Minion cores)
Each level adds resources that are shared by the units it contains. The device contains 34 Minion Shires, which together form the Minion Shire array (1.2.4. Minion Shire Array).
[image: images/ch01/fig-hierarchy.png]
Figure 1. ET-Minion hierarchy
1.2.1	ET-Minion Core
The ET-Minion is a dual-threaded, in-order, single-issue 64-bit RISC-V core that implements RV64IMFC. Its main features are:
· Two hardware threads (harts)
· 4 KB private L1 data cache, partly configurable as scratchpad memory
· Vector processing unit (VPU) with eight identical lanes operating in lock-step. Each lane contains:
· Floating-point multiply-add unit (FMA): one 32-bit or two 16-bit operations
· Two integer multiply-add units (IMA): four 8-bit multiply-accumulates each
· Integer unit (INT)
· Transcendental unit (TRANS)
· Esperanto instruction extensions for vector, tensor, atomic, message, cache-management and fast-synchronization operations
The core consists of four top-level blocks, shown in Figure 2:
· Front end (FE)
· Integer pipeline
· L1 data cache and scratchpad
· VPU
[image: images/ch01/fig-et-minion.png]
Figure 2. ET-Minion core
1.2.2	Neighborhood
A Neighborhood groups eight ET-Minion cores that share the following resources. In Figure 3, the L0 micro-caches are labeled "I-Cache".
· L1 instruction cache: 32 KB, organized as 128 sets × 4 ways with 64-byte lines. It is shared by all eight cores, and its data RAMs are located outside the Neighborhood.
· L0 micro-caches: two, each shared by four cores. Each holds 16 fully associative cache lines, sits between its cores and the L1 instruction cache, and accesses the L1 instruction cache on a miss.
· Page-table walkers (PTWs): two, each shared by four cores. Each PTW serves the data caches of its four cores and the instruction-cache side.
· Request/response path: a single path to the memory hierarchy outside the Neighborhood. Requests from the eight data caches, the instruction cache, the two PTWs and, the cooperative TensorLoad/TensorStore units are arbitrated into (256-bit internally which is converted to a 512-bit ET-Link bus).
· Performance monitoring unit (PMU): twelve 64-bit event counters shared by the eight cores.
Eight counters count ET-Minion events and four count Neighborhood events.
· Cooperative TensorLoad: coalesces the TensorLoad requests that several cores issue for the same address into a single memory request, and delivers the one response back to every cooperating core. Cores in all four Neighborhoods of a Minion Shire can cooperate; one Neighborhood acts as master and sends the combined request.
· Cooperative TensorStore: combines the partial writes of cooperating cores into one Shire Cache write, and replicates the acknowledgement to every core that took part. Cores cooperate in two fixed groups, cores 0 to 3 and cores 4 to 7, in one of three modes:
· Quad-128: 128 bits from each of four cores, forming a full 512-bit cache line
· Pair-256: 256 bits from each of two cores, forming a full 512-bit cache line
· Pair-128: 128 bits from each of two cores, forming half a cache line
· Each core holds its request until every core of the group has presented one, so operations of different modes cannot mix.
· Fast Local Messaging Network (FLN): carries messages between cores of the same Neighborhood directly, instead of sending them out through the request path and back in through the response path. Connections are not all-to-all; they follow the pattern used by the tensor reduction instructions, and a message arriving over this network takes priority over the other responses to that core.
· Fast local barrier (FLB) path
· Neighborhood ESRs
· Interrupts: routes the external, timer and software interrupt lines to the cores, and delivers the inter-processor interrupts (IPIs). A software write to a Shire ESR raises a machine software interrupt for a hart, or a redirect IPI that sends the selected harts to the PC held in the Neighborhood ipi_redirect_pc ESR.
[image: images/ch01/fig-neighborhood.png]
Figure 3. Neighborhood
1.2.3	Minion Shire
A Minion Shire groups four Neighborhoods (Figure 4). It also contains:
· Shire Cache: 4 MB, in four 1 MB banks. Programmable ESRs divide the cache into three kinds of partition:
· L2 cache, private to the Shire
· Slice of the chip-wide distributed L3 cache
· Scratchpad memory
· Crossbar: Request and response crossbars connect four Neighborhoods and the RBOX port to the four Shire Cache banks and the UC block. Each Neighborhood has one request and response port into the Shire Cache, and each bank accepts at most one request per cycle. The crossbar also connects the Neighborhoods to the un-cached (UC) block.
· Uncached (UC) block: receives the Neighborhood requests that are not sent to the Shire Cache banks. It handles uncacheable accesses, contains the fast local barrier (FLB) and fast local credit counter (FCC) units, and delivers messages sent between ET-Minion cores of different Shires.
· ESR banks: the Esperanto System Registers (ESRs) configure the blocks in the Shire.
· NoC interface: L2 misses and uncacheable accesses leave the Shire here, bound for other Shires or the memory controllers.
[image: images/ch01/fig-minion-shire.png]
Figure 4. Minion Shire
1.2.4	Minion Shire Array
The 34 Minion Shires, 1,088 ET-Minion cores in total, form the Minion Shire array. The roles of the Shires are assigned by software:
· Compute: 32 Minion Shires operate in parallel as the compute array.
· Master (management): one Minion Shire receives work and distributes it to the compute array.
· Spare: one Minion Shire.
All Minion Shires are identical in hardware, so any Minion Shire can take any of these roles.
1.3	ET-Maxion and Service Processor
In addition to the ET-Minion cores, the device contains two other core types. Both are located in the I/O Shire (1.4.4. I/O Shire). This document does not describe them beyond this section.
1.3.1	ET-Maxion Cores
The ET-Maxion is a single-threaded, superscalar, out-of-order 64-bit RISC-V core intended for management and general-purpose tasks. The device contains four identical ET-Maxion cores. Together with a 4 MB shared L2/L3 cache they form the Maxion Neighborhood, and a system bus and coherency hub in the I/O Shire connects them. Figure 5 shows the ET-Maxion pipeline.
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Figure 5. ET-Maxion pipeline
1.3.2	Service Processor
The Service Processor (SP) is a single-threaded ET-Minion core without the vector/tensor extensions. It has its own ROM and a 1 MB scratchpad SRAM, but none of the Neighborhood or Shire shared resources.
· Boot. The SP is the first major block released from reset. It executes the boot code from ROM and initializes the device interfaces, including DDR, PCIe and USB.
· Run time. It provides management services for the whole device.
· Access. The SP can access every resource on the device, and some resources are accessible only to it.
The I/O Shire also contains a hardware root of trust, and six secure mailboxes for communication between four agents:
· Service Processor
· Master Minion Shire
· ET-Maxions
· PCIe host
1.4	Mesh Network-on-Chip
The mesh NoC is the top-level interconnect of ET-SoC-1 and connects all Shires. Figure 6 shows the device with the Shire array on the mesh, the external memory and PCIe interfaces, and the peripheral, Service Processor and debug networks.
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Figure 6. ET-SoC-1 block diagram
1.4.1	Mesh Topology and Mesh Stops
The mesh is organized as an 8 × 6 grid, and each Shire attaches to it at a mesh stop. The Memory Shires occupy the east and west edges, four on each side, which leaves the corners of the grid unoccupied. The result is 44 mesh stops, listed in Table 2.
Table 2. Shires on the mesh
	Shire
	Count
	Contents

	Minion Shire
	34
	32 ET-Minion cores and a 4 MB Shire Cache

	Memory Shire
	8
	LPDDR4X memory controller

	PCIe Shire
	1
	PCIe controllers and PHY

	I/O Shire
	1
	ET-Maxions, Service Processor and peripherals

	Total
	44
	


1.4.2	Memory Shires
Each Memory Shire contains a 32-bit LPDDR4X PHY and two memory controllers, each driving one 16-bit channel achieving 4,266 MT/s/channel. The Memory Shires also support global atomic operations.
1.4.3	PCIe Shire
The PCIe Shire contains two dual-mode PCIe Gen4 controllers that share an 8-lane PHY. It supports three lane configurations:
· Single 8-lane endpoint or root complex
· Single 4-lane endpoint or root complex
· 4-lane endpoint together with a 4-lane root complex
The interface is normally factory-configured as an endpoint.
1.4.4	I/O Shire
The I/O Shire contains the ET-Maxions and the Service Processor (1.3. ET-Maxion and Service Processor). It also contains the device peripherals, which are grouped on three networks according to which agents may access them.
· Service Processor network. Accessible only to the SP. It contains:
· SPI, including the boot-flash controller
· I2C, including the link to the external power-management controller
· UART, including the SP console
· GPIO, timers, watchdog and boot control
· Peripheral network. Shared by the SP, the ET-Maxions and the master Minion Shire. It contains:
· eMMC, USB 2.0 OTG, I2C/SMBus, I3C, SPI and UART
· GPIO, timers and watchdog
· Debug network. Provides debug access through JTAG and a USB 2.0 device port.
1.5	ET-SoC-1 Accelerator Card
ET-SoC-1 operates as an accelerator attached to a host system over PCI Express. It is mounted on a PCIe add-in card (Figure 7) with the following features:
· PCIe x16 card-edge connector, with an 8-lane Gen4 interface to ET-SoC-1
· ET-SoC-1 soldered to the card
· Four LPDDR4X devices forming a 256-bit memory interface
· 64 GB eMMC flash memory
· USB connectors for the ET-SoC-1 device and debug ports and for a UART interface, and a JTAG connector
· DIP switches that select the boot options
Multiple ET-SoC-1 devices can also be integrated on a single card.
[image: images/ch01/fig-pcie-card.png]
Figure 7. ET-SoC-1 PCIe card
2	ET-Minion Core
2.1	Core Overview
This section describes the internal organization of the ET-Minion core: its block partitioning, hardware threads and instruction flow. The features of the core and its position in the ET-Minion hierarchy are summarized in 1.2.1. ET-Minion Core.
The ET-Minion is a dual-threaded, in-order, single-issue 64-bit RISC-V core that implements RV64IMFC with the Esperanto instruction extensions. It is implemented in minion_top and consists of four units: the Front End, the integer pipeline, the L1 data cache and the VPU. The core fetches instructions from the Neighborhood L0 micro-cache and accesses memory through the Neighborhood memory path; it has no instruction cache of its own.
2.1.1	Block Partitioning
The ET-Minion core is implemented in minion_top (Figure 2). minion_top contains two blocks: core_top, which holds the Front End, the integer pipeline, the L1 data cache and the debug APB slave, and vpu_top, the vector processing unit. Table 3 lists the blocks.
Table 3. ET-Minion core blocks
	Block
	Module
	Function

	Front End
	frontend_top
	Fetches instructions for both threads from the Neighborhood L0 micro-cache, expands compressed instructions, decodes them for the integer pipeline and the VPU, and issues one instruction per cycle to the integer pipeline (2.2. Front End).

	Integer pipeline
	intpipe_top
	In-order, single-issue pipeline with the stages ID, EX, GSC, TAG, MEM and WB. Contains the integer register file, ALU, multiply/divide unit, integer, FP and mask scoreboards, and the CSRs. Redirects the Front End on a change of control flow.

	Data cache
	dcache_top
	4 KB private L1 data cache, partly configurable as scratchpad memory. Contains the data TLB, PMA check, miss handling, replay queue, store merge, atomic (AMO) forwarding to L2 through the miss handler’s UC flow, scratchpad controller, write-back unit, cache management, tensor-load and reduce units, and the interface to the Neighborhood memory path.

	APB slave for debug registers
	minion_debug_apb_slv
	APB slave for debug access to the core, including writes to the debug program buffer.

	VPU
	vpu_top
	Vector processing unit with a control block and eight identical lanes. Executes floating-point, packed-integer, transcendental and tensor operations.


2.1.2	Hardware Threads
The core runs two hardware threads (CORE_NR_THREADS = 2). Each thread has its own architectural state; the pipeline and execution units are shared, and instructions of the two threads are interleaved in the pipeline.
Table 4. Per-thread and shared resources
	Per thread
	Shared by both threads

	Fetch PC, thread buffer and instruction FIFO in the Front End
	Front End request port, decoders and thread scheduler

	32 x 64-bit integer registers, in one register file indexed by thread
	Integer pipeline, ALU and multiply/divide unit

	32 vector registers, (also the FP f-registers), 256 bits wide, held as a 32-bit slice in each lane’s RF, which are indexed by the thread number. Eight 8-bit mask registers.
	VPU control and execution units

	CSR state, interrupt inputs and debug state
	L1 data cache and scratchpad


Each thread is enabled by its corrseponding bit of the enabled input of minion_top. minion_top registers enabled once, and the integer pipeline and debug logic uses this registered copy directly. The Front End regsisters it twice more, so that it can detect the edges of the enable and turn each rising and falling edge into a one-cycle enable of disable event (Section 2.2.6.3). When a thread is enabled, it starts fetching at reset_vector, which is the same for both threads.
The Front End selects one thread per cycle for issue to the integer pipeline. The integer pipeline can stall each thread independently, for example on WFI, a fence, a scoreboard hazard, or while the other thread holds exclusive mode. As a result, the Front End sees a change of enabled two cycles later than the integer pipeline does.
2.1.3	Instruction Flow Through the Core
The Front End fetches instructions for both threads from the Neighborhood L0 micro-cache, expands compressed instructions, decodes them, and presents one instruction per cycle to ID, the first stage of the integer pipeline. The integer pipeline executes the instructions in order and passes memory operations to the data cache and vector operations to the VPU. In the opposite direction, the integer pipeline redirects the Front End to a new fetch address after a branch misprediction, exception or other change of control flow, and stalls a thread that must not issue.
[image: images/ch02/fig-fe-in-core.png]
Figure 8. Front End in the ET-Minion core
2.1.4	Interfaces to the Neighborhood
Table: ET-Minion core interface groups.
2.1.5	Clocks, Resets and Power
2.1.6	Debug Support
2.2	Front End
2.2.1	Overview
The Front End (frontend_top) supplies instructions to the ET-Minion core. It sits between the Neighborhood L0 micro-cache and the ID stage of the integer pipeline. It holds the program counter of each of the two threads and fetches 32-byte instruction blocks from the L0 micro-cache. It then extracts the instruction, expands compressed instructions to 32 bits and decodes them for both the integer pipeline and the VPU. It delivers one decoded instruction per cycle to ID, from either thread. The core has no instruction cache of its own. Each L0 micro-cache is shared by four ET-Minion cores, eight threads in all, so the design of the Front End is driven by the need to hide the latency of shared fetch path.
The Front End is built around the following four concepts:
1. Fetch is double-buffered: each thread has a thread buffer with two 256-bit entries, each holding half a cache line, so the next block can be requested while the current one is being consumed.
1. Each thread has at most one fetch request in flight: the L0 micro-cache answers every accepted request, hit or miss, after a fixed latency, so a thread recognizes its own by timing alone, without a thread identifier. On a miss the thread sleeps until the L0 micro-cache reports that a fill has completed, and then retries.
1. Instructions are decoded before they are queued: one integer decoder and one VPU decoder, shared by both threads, decode in F7, and each thread has a two-entry instruction FIFO that holds decoded instructions until ID accepts them. This moves decode out of the ID stage and lets a thread keep fetching while ID serves the other thread.
1. The two threads are independent: each thread fetches, sleeps, stalls and restarts on its own. They share only the fetch request port, the decoders and the issue slot into ID, and the thread scheduler alternates between them when both are eligible.
The Front End is a pipeline of eight stages, F0 to F7. F1 to F5 overlap the L0 micro-cache pipeline. With an L0 hit and no competing requests, the first instruction of a block reaches ID nine cycles after it is requested. The first target instruction reaches ID ten cycles after a redirect, and the first instruction reaches ID eleven cycles after a thread is enabled.
The integer pipeline controls the Front End through two per-thread signals. A redirect (f0_core_req_valid, f0_core_req) flushes the thread and restarts fetch at a new PC. It is used for mispredictions, exceptions, replays, interrupts and debug-mode transitions. A stall (id_core_stall) stops the thread from being scheduled, for example on WFI, a fence, a CSR access that must wait, or a scoreboard hazard. The Front End attaches the fetch status to each instruction: page and access faults, bus and ECC errors, and a replay flag for uncacheable fetches issued while older instructions are still in flight. The integer pipeline acts on this status in ID.
The Front End also starts and stops threads through their enable inputs and reset vector. It supports debug in two ways: it generates the placeholder instruction on which a halt is taken, and it lets entry 0 of a halted thread’s buffer serve as the debug program buffer. Each thread buffer runs on its own gated clock; a chicken bit disables the gating.
Table 5 lists the submodules and Figure 9 shows how they are connected. The sections that follow cover the interface (2.2.2. Interface), the pipeline stages (2.2.3. Pipeline Stages), the fetch protocol with the L0 micro-cache (2.2.4. Interaction with the L0 Micro-Cache), the thread buffer (2.2.5. Thread Buffer and 2.2.6. Entry Invalidation, Redirect and Thread Start), decode (2.2.7. Decoders), the instruction FIFO (2.2.8. Instruction FIFO), the thread scheduler (2.2.9. Thread Scheduler), and halt and debug support (2.2.10. Halt and Debug Program Buffer).
Table 5. Front End submodules
	Submodule
	Instances
	Function

	Thread buffer (frontend_thread_buffer)
	2, one per thread
	64-byte instruction buffer and the thread’s program counter. Issues fetch requests to the L0 micro-cache.

	RVC expander (frontend_rvc_expander)
	2, one per thread buffer
	Expands compressed (RVC) instructions to 32 bits.

	Request arbiter (arb_lru_data)
	1
	2:1 LRU arbiter. Selects the thread whose fetch request is sent to the L0 micro-cache.

	Integer decoder (intpipe_decode)
	1
	Decodes the instruction into integer-pipeline control signals.

	VPU decoder (vpu_decoder)
	1
	Decodes the instruction into VPU control signals.

	Instruction FIFO
(inline generate block)
	2, one per thread
	Two-entry queue of decoded instructions waiting for the integer pipeline.

	Thread scheduler (frontend_thread_sched)
	1
	Selects the thread whose instruction is presented to the integer pipeline.


[image: images/ch02/fig-fe-top-blocks.png]
Figure 9. Front End block diagram
2.2.2	Interface
This section defines the boundary of frontend_top. Section 2.2.2.1 lists its ports in six groups. The system group has the clock, the warm and debug resets and the clock-gating chicken bit. Thread control has the thread enables, the reset vector and the virtual-memory status of each thread. The L0 micro-cache group has the fetch request and response and the fill-done signal. The integer-pipeline group has the per-thread redirect and stall inputs. The output group carries the instruction and it’s decoded data to ID. The debug group has the halt, halted and program-buffer signals. For each port the table gives the net it connects to in core_top.
Section 2.2.2.2 gives the field layout and bit width of each packed structure that crosses these ports. These are the fetch request and response, the virtual-memory status, the redirect, the instruction delivered to ID, the instruction FIFO entry, and the two decoded control words. Section 2.2.2.3 lists the defines that set the number of threads, the buffer geometry and the PC width.
2.2.2.1	I/O Signals
Table 6 lists the ports of frontend_top. Connected to gives the signal in core_top. A width of 2 denotes one bit per thread.
Table 6. Front End I/O signals
	Signal
	Dir
	Width / type
	Connected to
	Description

	System

	clock
	in
	1
	clock
	Core clock. Each thread buffer derives a gated clock from it.

	reset
	in
	1
	reset_w
	Warm reset. Synchronous.

	reset_debug
	in
	1
	reset_d
	Debug reset. Clears the program-buffer control and, while the thread is halted, refills the program buffer with EBREAK.

	chicken_bit
	in
	1
	chicken_bit_frontend
	Disables Front End clock gating. Driven by the min_frontend_clock_gate_disable chicken bit.

	Thread control

	f0_thread_enabled
	in
	2
	enabled
	Thread enable. A rising edge starts fetch at the reset vector; a falling edge stops fetch.

	f0_reset_vector
	in
	48
	reset_vector
	Fetch address after reset or thread enable.

	vm_status
	in
	2 x minion_vm_status
	vm_status
	Virtual-memory status of each thread, forwarded with every fetch request.

	Fetch request to the L0 micro-cache

	f1_icache_req_valid
	out
	1
	icache_req_valid
	The F1 I-cache request register holds a request.

	f1_icache_req
	out
	frontend_icache_req
	icache_req
	Fetch request: thread, VM status and address.

	f1_icache_req_ready
	in
	1
	icache_req_ready
	The Neighborhood accepts the request in this cycle.

	Fetch response from the L0 micro-cache

	f5_icache_resp_valid
	in
	1
	icache_resp_valid
	A response is present. It carries no thread identifier.

	f5_icache_resp_miss
	in
	1
	icache_resp_miss
	The response is a miss and carries no instruction data.

	f5_icache_resp
	in
	icache_frontend_resp
	icache_resp
	32-byte block and status.

	f6_icache_fill_done
	in
	1
	icache_fill_done
	The L0 micro-cache has completed a line or translation fill.

	Redirect and stall from the integer pipeline

	f0_core_req_valid
	in
	2
	id_core_fe_req_valid
	Redirect. Flushes the thread and restarts fetch at f0_core_req.pc.

	f0_core_req
	in
	2 x minion_fe_req
	id_core_fe_req
	Redirect PC, speculation status and debug-mode transition.

	id_core_stall
	in
	2
	id_core_fe_stall
	Thread must not issue. Raised for WFI, CSR accesses that are replayed until a resource is ready (e.g., TensorWait, tensor ops, FCC), a fence, exclusive mode held by the other thread, and integer or FP scoreboard stalls. The WFI/CSR term is suppressed while debug mode or halt request is active.

	Instruction to the integer pipeline (ID)

	id_inst_valid
	out
	1
	id_fe_core_resp_valid
	The instruction presented to the integer pipeline is valid.

	id_inst_ready
	in
	1
	id_core_fe_resp_ready
	The integer pipeline is ready to accept the instruction.

	id_inst_thread_id
	out
	1
	id_fe_core_resp_thread_id
	Thread of the instruction.

	id_inst_data
	out
	frontend_core_resp
	id_fe_core_resp
	Instruction, PC and fetch status.

	id_intpipe_ctrl
	out
	minion_control
	id_intpipe_ctrl
	Integer decode.

	id_vpu_decoder_sigs
	out
	vpu_ctrl_sigs_t
	id_vpu_decoder_sigs
	VPU decode. Valid only for VPU instructions.

	id_vpu_core_ctrl
	out
	vpu_minion_id_ctrl
	id_frontend_vpu_ctrl
	VPU and mask register usage, for hazard checks in the integer pipeline.

	Debug

	halt
	in
	2
	debug_in_core.halt
	A halt request is pending.

	halted
	in
	2
	debug_out.halted
	The thread is in debug mode.

	debug_ffb_wdata
	in
	64
	debug_ffb_wdata
	Program-buffer write data.

	debug_ffb_en
	in
	4
	debug_ffb_en
	Program-buffer word write enables.

	debug_ffb_thread_sel
	in
	1
	debug_ffb_thread_sel
	Thread whose program buffer is written.

	debug_ffb_exec
	in
	2
	debug_ex_program_buffer
	Start executing the program buffer.


2.2.2.2	Data Structures
Table 7. frontend_icache_req: fetch request (58 bits)
	Field
	Width
	Description

	thread_id
	1
	Requesting thread.

	vm_status
	minion_vm_status
	Virtual-memory status of the thread (Table 8).

	addr
	49
	Fetch address. The L0 micro-cache returns the aligned 32-byte block that contains it.


Front End addresses are 49 bits wide: the 48-bit virtual address and one additional bit that allows a non-canonical 64-bit address to be represented.
Table 8. minion_vm_status: virtual-memory status (8 bits)
	Field
	Width
	Description

	prv
	2
	Current privilege level.

	mprv, mpp, sum, mxr
	1, 2, 1, 1
	Corresponding mstatus fields.

	debug
	1
	Thread is in debug mode.



Table 9. icache_frontend_resp: fetch response (261 bits)
	Field
	Width
	Description

	data
	256
	32-byte instruction block.

	page_fault
	1
	Instruction page fault.

	access_fault
	1
	Instruction access fault.

	cacheable
	1
	Block is in a cacheable region.

	bus_err
	1
	Bus error on the line.

	ecc_err
	1
	ECC error on the line.



Table 10. minion_fe_req: redirect (52 bits)
	Field
	Width
	Description

	pc
	49
	New fetch PC.

	speculative
	1
	Thread has older instructions in the integer pipeline. Driven every cycle, independently of f0_core_req_valid. Used for replay (Section 2.2.5.6).

	debug_info.halt
	1
	Redirect enters debug mode.

	debug_info.resume
	1
	Redirect leaves debug mode.



Table 11. frontend_core_resp: instruction to the integer pipeline (89 bits)
	Field
	Width
	Description

	pc
	49
	PC of the instruction.

	inst_bits
	32
	Instruction. Compressed instructions are delivered expanded.

	pf0, af0
	1 each
	Page fault / access fault on the entry holding the start of the instruction.

	pf1, af1
	1 each
	Page fault / access fault on the entry holding the upper half of an instruction that crosses entries.

	replay
	1
	Instruction must be replayed.

	rvc
	1
	Instruction was compressed.

	bus_error, ecc_error
	1 each
	Bus error / ECC error on the entry or entries holding the instruction.



Table 12. frontend_thread_data: instruction FIFO entry (179 bits)
	Field
	Width
	Description

	core_resp
	89
	Instruction and fetch status (Table 11).

	vpu_ctrl_sigs
	45
	VPU decode (vpu_ctrl_sigs_t).

	intpipe_ctrl
	45
	Integer decode (minion_control).



Table 13. Decoded control words
	Structure
	Width
	Content

	minion_control
	45
	Legal instruction; software-emulated (M-code) instruction; branch, JAL, JALR; integer source reads and destination write; ALU operand selects, function and width; immediate format; memory operation, command and size; FP/VPU destination write; mask register read/write; multiply/divide; CSR command; fence; global memory access; gather/scatter; graphics; implicit use of x31.

	vpu_ctrl_sigs_t
	45
	VPU function; execution unit (TxFMA, shift/swizzle, transcendental ROM); conversion and load/store type; source, third-source and destination reads and write; mask register reads; operand swaps; scalar or packed; data type; integer-register transfer; rounding; FP flag update.


2.2.2.3	Configuration Parameters
Table 14. Front End configuration parameters
	Define
	Value
	Description

	CORE_NR_THREADS
	2
	Threads per core.

	FE_FETCH_BUFFERS
	2
	Thread-buffer entries per thread.

	FE_FETCH_READ_SIZE
	256
	Bits per fetch block and per entry.

	FE_FETCH_PTR_SIZE
	5
	Read-pointer width: 1 entry bit and 4 halfword bits.
log2(FE_FETCH_VALID_INST_SIZE * FE_FETCH_BUFFERS) = log2(16 * 2) = 5

	PC_SIZE_EXT
	49
	Front End PC width.


2.2.3	Pipeline Stages
This section describes the eight Front End stages, F0 to F7, and how they line up with the L0 micro-cache pipeline. Two activities run in parallel and meet in the thread buffer. Fetch runs from F0 to F6: a thread’s request is arbitrated and sent in F0, waits for acceptance in F1, is looked up in F1 to F5, and the response is written into the thread buffer in F6; a miss writes nothing and the thread goes to sleep. In F7 each thread pulls its next instruction out of its buffer and expands it if compressed. One thread’s instruction is decoded and placed in its FIFO. The scheduler presents one thread’s FIFO head to the integer pipeline each cycle
Fetching and extracting are independent: a thread keeps extracting instructions from a filled buffer entry while its next request is still in F0-F5.
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Figure 10. Front End pipeline
F0 Stage
The F0 stage receives instruction-block requests from both thread buffers and decides which one gets access to the L0 micro-cache using a 2:1 LRU arbiter. The selected request is registered and sent to the L0 micro-cache through the Neighborhood interface. This stage also handles the enabling and disabling of threads and redirect requests from the integer pipeline, for example the new address after a mispredicted branch.
F1–F5 Stage
The selected request is held in F1 until the L0 micro-cache accepts it, which happens at the earliest in the second F1 cycle. The thread then waits for the response. The L0 micro-cache always responds to an accepted request, whether it is a hit or a miss, with a fixed five-cycle latency: counting the cycle in which it accepts the request as the first cycle, the response is returned in the fifth cycle, in F5 (Figure 12).
F6 Stage
The response from the L0 micro-cache is checked. If it is a hit, the instruction block is stored in the buffer of the thread that issued the request. If it is a miss, nothing is stored, and the thread waits for the cache to be filled. Instruction reading is independent of the fetch request: whenever a buffer entry holds instructions, the thread reads its next instruction, expands it if it is compressed, and passes it on for decoding, in parallel with any request in F0 to F5.
F7 Stage
This stage selects which thread’s instruction is read from its buffer. The selected instruction is decoded and stored, along with its control signals, in that thread’s FIFO. The thread scheduler decides which thread’s FIFO issues an instruction to the integer pipeline in the next cycle. If both threads are eligible, they are selected in round-robin order; otherwise, the eligible thread is selected.
With an L0 hit and no competing requests, the first instruction of a block reaches ID nine cycles after its request is issued in F0.
2.2.4	Interaction with the L0 Micro-Cache
This section describes the fetch protocol between the Front End and the L0 micro-cache, from the Front End side. It covers the following four things:
1. How a request is arbitrated and accepted: by the 2:1 LRU arbiter and F1 request register in the core, then by the 8:1 arbiter of the Neighborhood.
1. The fixed response timing, and how a thread recognizes its own responses with a token tracker, since responses carry no thread identifier.
1. The miss, sleep and fill-done protocol, and why its timing guarantees that no wake-up is lost.
1. How a redirect cancels requests already in flight, including one still waiting in the F1 register.
Each L0 micro-cache serves the eight threads of four ET-Minion cores. Figure 11 shows the request and response path of one core. The Neighborhood side of the interface is described in 3.2. Front End – I-Cache Interface.
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Figure 11. Front End to L0 micro-cache request and response path
2.2.4.1	Request Arbitration and Acceptance
A fetch request passes through the following steps:
1. 2:1 LRU arbiter, F0. Selects between the two threads of the core. With two clients the grant alternates when both threads request. The priority is updated on every grant.
1. F1 I-cache request register (f1_icache_req). Holds the granted request until the Neighborhood accepts it with f1_icache_req_ready. The register accepts a new request when it is empty or its current request is accepted in the same cycle; otherwise the 2:1 arbiter issues no grant.
1. 8:1 LRU arbiter, Neighborhood. The request is first captured in a per-thread request register, then arbitrated against the other seven threads served by the same L0 micro-cache. The grant of this arbiter is returned as f1_icache_req_ready. Because of the capture register, a request is accepted at the earliest in its second F1 cycle.
2.2.4.2	Response Timing and Ownership
The L0 micro-cache has a five-stage pipeline and returns exactly one response per accepted request, from its last stage, for a hit and for a miss alike. The response reaches the Front End in F5.
The response carries no thread identifier. Each thread buffer identifies its responses by position in time: when its request is granted, the thread inserts a token (a valid bit and the reserved entry number) into its own F1–F6 tracker. The token remains in F1 until the request is accepted and then advances one stage per cycle. A response registered in F6 together with a valid token belongs to that thread, and the token selects the entry to be written. The response and fill-done signals are registered in frontend_top and broadcast to both thread buffers.
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Figure 12. Request and hit response
In Figure 12 the request is issued in cycle 1, accepted in cycle 3, and the block returns in cycle 7. It is written in cycle 8; the first instruction of the fetched block is in the F7 stage in cycle 9 and in the ID stage in cycle 10.
2.2.4.3	Miss Handling and Fill Done
A miss response has the same timing as a hit and carries no data. On a miss the thread writes nothing, keeps its fetch PC and enters a sleep state (f0_miss_pending) in which it issues no requests.
On completion of a line fill from the L1 instruction cache, or of a translation fill, the L0 micro-cache pulses f6_icache_fill_done. The signal is broadcast to all threads of the L0 micro-cache and carries no address. Every sleeping thread wakes and retries; a thread whose line is still absent misses again and sleeps until the next fill. A redirect, a thread disable or a pending halt also clears the sleep state.
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Figure 13. Miss, sleep and retry
In Figure 13 the miss response arrives in cycle 7 and the thread sleeps from cycle 9. Fill done arrives in cycle 11, is registered, and the thread retries in cycle 12.
Fill done is issued one cycle after the response slot. A request that looks up the L0 micro-cache while a fill is being written still misses, and its response is the last miss that the fill can cause. Issuing fill done one cycle after that response, and registering it again in the Front End, ensures that every thread has entered the sleep state before the wake-up arrives. A wake-up that arrived first would be lost, and the thread would wait for an unrelated fill.
2.2.4.4	Request Cancellation
A redirect invalidates the thread’s tokens in F2 to F5 and suppresses the F6 write, so the responses of in-flight requests are discarded.
A request still waiting in the F1 I-cache request register cannot be withdrawn: the register is shared and the Neighborhood already holds a copy. The thread records the cancellation and does not advance the token when the request is accepted. The I-cache lookup is performed and its response is discarded. The thread’s new request is issued only after the cancelled request has been accepted.
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Figure 14. Redirect while a request waits in F1
In Figure 14 the redirect arrives in cycle 3 while the request waits in F1. The cancellation is held until the request is accepted in cycle 5; no token enters F2. The new request is issued in cycle 6 and accepted in cycle 8.
2.2.5	Thread Buffer
The thread buffer (frontend_thread_buffer) holds almost all of a thread’s Front End state; there is one buffer per thread. This section describes how the buffer stores instructions: two 256-bit entries in a latch register file with a 32-bit, wrap-around read port. It then describes the state kept for each entry, the fetch PC and how it is updated, and the conditions under which the thread requests a new block. It also shows how an entry is reserved and written.
The section then shows the instruction side: how the read pointer extracts one instruction per cycle, including instructions that cross from one entry to the other and the bypass from incoming data. It then covers how the RVC expander turns compressed instructions into 32-bit ones, and which fault, error and replay status is attached to each instruction on its way to the integer pipeline.
[image: images/ch02/fig-fe-thread-buffer-flow.png]
Figure 15. Thread buffer operation
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Figure 16. Thread buffer pipeline
2.2.5.1	Buffer Entries
The instruction buffer has two entries of 256 bits (32 bytes). An entry holds one fetch block: eight 32-bit instructions, sixteen compressed instructions, or a combination. Two entries allow the next block to be fetched while the current block is consumed.
The entries are implemented as one latch-based register file with two ports:
· Write port, 256 bits. Writes a complete block into one entry, with one write enable per 32-bit word.
· Read port, 32 bits. Addressed by the 5-bit read pointer buffer_ptr: bit 4 selects the entry, bits 3:0 select a halfword within it. The read returns the 32 bits starting at that halfword.
The read port wraps around: halfword 15 of one entry is followed by halfword 0 of the other. The entries therefore form a ring of 32 halfwords, and a 32-bit instruction that starts in the last halfword of an entry is read in one access.
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Figure 17. Thread-buffer entries and read pointer
Table 15. Thread-buffer entry state
	State
	Description

	Empty flag
	Entry holds no instruction still to be sent. Set for both entries at reset.

	Block address
	Address of the instruction block held in the entry (buffer_pc). Only the words from this address onward are written, extraction in the entry starts at this address, and it provides the upper PC bits of every instruction read from the entry.

	Fault flags
	Page fault and access fault of the block.

	Error flags
	Bus error and ECC error of the block.

	Cacheable flag
	Block is in a cacheable region. Used for replay.


2.2.5.2	Program Counter
Each thread buffer holds a 49-bit fetch PC, the address of the next block to request. It is updated as listed in Table 16.
Table 16. Fetch PC update
	Event
	New fetch PC

	Reset, or thread enabled
	f0_reset_vector, sign-extended.

	Block written into an entry
	Start of the next aligned 32-byte block.

	Redirect (highest priority)
	f0_core_req.pc.


Only the first block after a reset or redirect can start within a 32-byte block; all later blocks are aligned. A miss does not change the fetch PC, so the same address is requested again after the fill.
The PC of each extracted instruction is formed from the upper bits of its entry’s block address and the halfword position of the read pointer.
2.2.5.3	Request Generation and Entry Fill
A thread issues a request in F0 when all conditions in Table 17 are met.
Table 17. Request conditions
	Condition
	Reason

	Thread enabled, and not in the enable cycle
	Reset vector is loaded at the end of the enable cycle.

	No redirect in the current cycle
	Redirect PC is loaded at the end of the cycle.

	Thread not sleeping, or registered fill done in this cycle
	After a miss the thread waits for a fill; the request is issued in the cycle the registered fill done arrives.

	No request of the thread in F1 to F6
	At most one request per thread is in flight, which keeps responses in order and allows ownership by timing.

	An entry is empty or is released in the current cycle
	The response cannot be stalled and must have a destination.

	No halt pending
	While a halt is pending the thread sends no request to the L0 micro-cache; it produces a placeholder instruction instead (Section 2.2.10.1).

	Not in reset; not executing the debug program buffer
	—


On a grant, the thread reserves an entry and records the fetch PC of the request as the entry’s block address. If both entries are empty, entry 1 is reserved.
Table 18 shows the entry sequence after a thread is enabled at address A. [m, n] gives the block number in entry 0 and entry 1; x denotes an empty entry.
Table 18. Entry fill sequence
	Step
	Event
	Entries

	1
	Thread enabled at address A.
	[x, x]

	2
	Block containing A written into entry 1; extraction starts at the halfword of A.
	[x, A>>5]

	3
	Entry 0 empty: the next block is requested when the first request completes.
	[(A>>5)+1, A>>5]

	4
	Last instruction of entry 1 extracted; entry 1 released.
	[(A>>5)+1, x]

	5
	Next block requested into entry 1; extraction continues in entry 0.
	[(A>>5)+1, (A>>5)+2]


A block write enables only the words from the word containing the request address to word 7. The register file requires its write-data enables one clock phase before the write; the thread computes them in F5 from its token and f5_icache_resp_miss, holds them in a phase latch, and applies the word write enables in F6.
2.2.5.4	Instruction Extraction
When both entries are empty, the read pointer is loaded in F5 with the halfword position of the request address within the reserved entry, so that extraction can start within a block. Afterwards the pointer advances with each extracted instruction.
An instruction is available when the entry it is read from is not empty. A 32-bit instruction that starts in halfword 15 requires both entries to be non-empty; the wrap-around read returns both halves, the pointer moves to halfword 1 of the other entry, and the first entry is released.
If the entry being read is empty but its block is written in the same cycle, the instruction is taken directly from the response data (bypass). The upper half of an instruction that crosses into an entry being written is bypassed in the same way. The first instruction of a block is therefore extracted in the cycle the block is written. The bypass does not check the destination entry of the response; with one request in flight per thread, the only block that can arrive is the one being waited for.
2.2.5.5	RVC Expander
The 32 bits read at the pointer are passed to the RVC expander (frontend_rvc_expander), a combinational RV64C decompressor:
· If bits [1:0] are not 11, the instruction is compressed. It is expanded to its 32-bit equivalent and the pointer advances by 16 bits.
· If bits [1:0] are 11, the instruction is 32 bits wide. It passes through unchanged and the pointer advances by 32 bits.
All instructions are therefore 32 bits wide after F6. The rvc bit of frontend_core_resp indicates a compressed instruction; the integer pipeline uses it to advance the PC by 2 instead of 4.
2.2.5.6	Fault and Error Status
Each instruction carries the status of the entries it was read from:
Table 19. Instruction fetch status
	Field
	Source

	pf0, af0
	Fault flags of the entry holding the start of the instruction.

	pf1, af1
	Fault flags of the entry holding the upper half of an instruction that crosses entries; zero otherwise.

	bus_error, ecc_error
	Error flags of the instruction’s entry, or of both entries for an instruction that crosses entries.

	replay
	Set when the entry’s block is not cacheable and f0_core_req.speculative indicates older instructions of the thread in flight. Captured when the instruction is written into the FIFO.


All status fields are forced to zero while the debug program buffer is executed.
2.2.6	Entry Invalidation, Redirect and Thread Start
This section describes the events that discard buffered instructions or restart fetch. Section 2.2.6.1 lists when a buffer entry is released: normally when its last instruction has been extracted, but also on a redirect, a thread disable or entry to debug mode. Section 2.2.6.2 describes a redirect from the integer pipeline: what triggers it, what it clears in each stage, and how long the thread takes to deliver its first target instruction. Section 2.2.6.3 describes how thread enable and disable events are derived from the enable input, how fetch starts at the reset vector, and what state a thread has after reset.
2.2.6.1	Entry Invalidation
An entry is released when its last instruction leaves F6, or when the whole buffer is flushed (Table 20).
Table 20. Entry release conditions
	Condition
	Entries released

	32-bit instruction at byte offset 28 of the entry is extracted
	This entry

	Compressed instruction at byte offset 30 is extracted
	This entry

	32-bit instruction at byte offset 30 is extracted (upper half in the other entry)
	This entry

	Redirect (f0_core_req_valid) or thread disable
	Both entries

	Entry to debug mode
	Both entries


A response that reports a fault or error marks the reserved entry non-empty even if no data is written, so that the fault is delivered to the integer pipeline with the next instruction read from that entry.
2.2.6.2	Redirect
The integer pipeline redirects a thread by asserting f0_core_req_valid with the new PC in f0_core_req.pc. Redirects are issued for branch and jump mispredictions, exceptions and returns from trap, replays, inter-processor interrupts, and entry to or exit from debug mode. Table 21 lists the effect in the redirect cycle.
Table 21. Effect of a redirect
	Stage
	Effect

	F0
	Fetch PC loaded with the redirect PC. No request in this cycle. Sleep state cleared.

	F1
	Request waiting in the F1 I-cache request register marked cancelled.

	F2–F5
	Tokens invalidated.

	F6
	No block written. Both entries released.

	F7
	Instruction discarded.

	FIFO
	Emptied. The thread is not eligible for scheduling in this cycle.


The target block is requested in the following cycle. Its first instruction reaches ID ten cycles after the redirect (Figure 18).
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Figure 18. Redirect to first target instruction
2.2.6.3	Thread Enable and Reset Vector
f0_thread_enabled is registered on entry to the Front End, and one-cycle enable and disable events are derived from its edges.
· Enable. The fetch PC is loaded with f0_reset_vector at the end of the enable cycle, and the first request is issued in the next cycle. The first instruction reaches ID eleven cycles after f0_thread_enabled rises (Figure 19).
· Disable. No further requests are issued, both entries are released and the sleep state is cleared. A fetch already in flight is not cancelled: its response is still written into its reserved entry. The instruction in F7 and the FIFO contents are not cleared. The thread is removed from the scheduler’s eligible set one cycle later. Because the scheduler defaults to thread 0, FIFO entries left by a disabled thread 0 can still be presented to ID. The eleven-cycle enable latency applies to a thread whose F7, FIFO and buffer are empty, for example the first enable after reset.
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Figure 19. Thread enable to first instruction
After reset, both entries are empty and the fetch PC holds the reset vector.
2.2.7	Decoders
This section describes the integer decoder (intpipe_decode) and the VPU decoder (vpu_decoder). Both are shared by the two threads and decode in F7, before the instruction is queued. It describes the control words the decoders produce, minion_control and vpu_ctrl_sigs_t, and how each decoder handles an encoding it does not recognize. It also describes the rule that selects which thread’s instruction is decoded in a cycle.
The section also explains how the VPU decode is used once the instruction reaches ID. The Front End does not issue to the VPU itself: the VPU control word goes directly to the VPU. The integer pipeline issues the instruction to the VPU and uses a summary of the control word for its FP and mask scoreboard checks
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Figure 20. Decoders, instruction FIFOs and thread scheduler
Both decoders are combinational look-up tables over the 32-bit instruction:
· Integer decoder. Produces minion_control (Table 13). An unlisted encoding is marked not legal, and the integer pipeline raises an illegal-instruction exception.
· VPU decoder. Produces vpu_ctrl_sigs_t and a flag that identifies VPU instructions. An unlisted encoding is a non-VPU instruction.
A thread is a decode candidate when it has an extracted instruction, its FIFO is not full and it is awake (2.2.9. Thread Scheduler). The decoded thread is selected as follows:
Table 22. Decode thread selection
	Candidates
	Thread decoded

	Thread 0 only
	Thread 0

	Thread 1 only
	Thread 1

	Both
	Thread not presented in ID in the current cycle

	None
	Thread not presented in ID in the current cycle


The instruction is written into the FIFO when the selected thread has an extracted instruction and its FIFO is not full; the awake condition affects only the selection.
The Front End does not issue instructions to the VPU. In ID, the VPU control word of the presented instruction (id_vpu_decoder_sigs) is sent directly to the VPU, bypassing the integer pipeline. The integer pipeline issues the instruction to the VPU in the same cycle, when the instruction is accepted in ID and decoded as an FP or VPU instruction, together with its thread and that thread’s fcsr rounding mode. The integer pipeline also receives a summary of the VPU control word (id_vpu_core_ctrl), with the VPU and mask register reads and writes of the instruction, for its FP and mask scoreboard checks.
2.2.8	Instruction FIFO
This section describes the two-entry instruction FIFO that each thread has (uses) between F7 and ID. The FIFO decouples fetch from issue. While ID is stalled or serving the other thread, the thread keeps extracting and decoding, and the FIFO holds the decoded instructions with their fetch status. The section covers what an entry holds and the pointer scheme that tracks occupancy. It explains why the storage is arranged for timing, as a fixed head register and a holding register, and gives the update rules. It also covers when the VPU control word is valid and how a redirect empties the FIFO.
The FIFO is written when its thread is selected for decode and read when the integer pipeline accepts the thread’s instruction (id_inst_valid, id_inst_ready and id_inst_thread_id). It uses 2-bit read and write pointers; it is full when the pointers differ only in the wrap bit and empty when they are equal.
The storage is organized for timing rather than as an indexed array. Entry 0 is always the head, whose content drives the ID outputs; entry 1 is a holding register. The ID multiplexer therefore selects between two fixed registers, one per thread.
Table 23. Instruction FIFO update
	Occupancy
	Event
	Update

	Empty
	Write
	Entry 0 ← new instruction

	One
	Write and read
	Entry 0 ← new instruction

	One
	Write
	Entry 1 ← new instruction

	One
	Read
	None; FIFO becomes empty

	Full
	Read
	Entry 0 ← entry 1


The VPU control word of an entry is written only for VPU instructions. For other instructions it retains the value of an earlier VPU instruction, so id_vpu_decoder_sigs and id_vpu_core_ctrl are valid only for VPU instructions.
A redirect empties the thread’s FIFO.
2.2.9	Thread Scheduler
The integer pipeline accepts one instruction per cycle from either thread. This section describes how the thread scheduler (frontend_thread_sched) chooses which thread’s FIFO head is presented to ID in the next cycle. It defines when a thread is awake (enabled and not stalled by the integer pipeline) and when it is ready (it has an instruction and is not being redirected). It gives the round-robin rule between eligible threads, including the default choice when neither thread is eligible. It then describes the handshake with ID: what drives the ID outputs, why the valid signal is not qualified with the stall, and what happens to an instruction that ID does not accept.
Awake
The thread is enabled and id_core_stall is deasserted. Awake is registered, so a stall affects scheduling one cycle after it is asserted.
Ready
The thread’s FIFO is not empty or is being written in the current cycle, and the thread is not being redirected. Including the write allows an instruction to pass from F7 to ID in consecutive cycles.
A thread that is awake and ready is eligible. The scheduler selects between eligible threads in round-robin order:
Table 24. Thread selection
	Thread 0 eligible
	Thread 1 eligible
	Selected

	Yes
	No
	Thread 0

	No
	Yes
	Thread 1

	Yes
	Yes
	Thread not selected previously

	No
	No
	Thread 0


The previous selection is updated only when at least one thread is eligible. The selection is registered and drives id_inst_thread_id in the next cycle.
The head of the selected thread’s FIFO drives id_inst_data, id_intpipe_ctrl, id_vpu_decoder_sigs and id_vpu_core_ctrl. id_inst_valid is asserted when that FIFO is not empty, and the integer pipeline accepts the instruction with id_inst_ready. id_inst_valid is not qualified with id_core_stall; the integer pipeline applies the stall. The thread in ID is reselected every cycle, so an instruction that is not accepted can be replaced by the other thread’s instruction in the next cycle; it remains at the head of its FIFO.
[image: images/ch02/td-fe-sched.png]
Figure 21. Round-robin issue with a stall
In Figure 21 both threads are eligible and alternate. id_core_stall of thread 1 is asserted in cycles 3 and 4, and thread 1 is not awake in cycles 4 and 5. Thread 0 is selected in cycles 3 to 5 and presented in ID in cycles 4 to 6; the selection alternates again from cycle 6.
2.2.10	Halt and Debug Program Buffer
This section describes the Front End’s two debug functions. Section 2.2.10.1 covers halt. The integer pipeline takes a halt only on a valid instruction in ID, so while a halt is requested the thread buffer generates a placeholder instruction instead of fetching, and passes it through the normal pipeline to ID.
Section 2.2.10.2 covers the debug program buffer. In debug mode, entry 0 of the halted thread’s buffer holds the instructions written by the debugger. The section describes how the buffer is prepared with EBREAK on entry to debug mode, how the debugger writes words into it and starts execution, and how a resume redirect ends program-buffer mode. It also shows which write data goes to which word, and why the last word always holds EBREAK.
2.2.10.1	Halt
The integer pipeline takes a halt on a valid instruction in ID. While halt is asserted for a thread, the thread buffer generates a placeholder instruction instead of fetching:
1. The thread follows the normal request conditions but does not bid for the request port. The request is treated as accepted internally, and its token enters the tracker.
1. The token passes through F1 to F6.
1. In F6 an entry write is forced without a response. The data is the last registered response data; fault and error flags are cleared, and the instruction is treated as 32 bits wide.
1. The placeholder passes through decode and the FIFO to ID, where the integer pipeline takes the halt.
The content of the placeholder is undefined. A pending halt also clears the sleep state.
2.2.10.2	Debug Program Buffer
In debug mode, entry 0 of the halted thread’s buffer is used as the program buffer: the debugger writes instructions into it and the thread executes them.
Table 25. Debug program-buffer sequence
	Step
	Operation

	Entry
	A redirect with debug_info.halt arrives; the thread stops fetching in the same cycle. In the next cycle both entries are released, the extracted instruction is discarded, and words 0 to 4 of entry 0 are written with EBREAK.

	Write
	The debugger writes the program buffer through debug_ffb_wdata, debug_ffb_en and debug_ffb_thread_sel (Table 26). The data and enables come together but the data is written into the entry in the cycle after the enables.

	Execute
	debug_ffb_exec resets the read pointer to halfword 0 of entry 0. In the next cycle entry 0 is marked non-empty and entry 1 empty, and instructions are extracted from word 0.

	Exit
	A redirect with debug_info.resume ends program-buffer mode; fetch restarts at the redirect PC.



Table 26. Program-buffer word mapping
	Word
	Write enable
	Data

	0
	debug_ffb_en[0]
	debug_ffb_wdata[31:0]

	1
	debug_ffb_en[1]
	debug_ffb_wdata[63:32]

	2
	debug_ffb_en[2]
	debug_ffb_wdata[31:0]

	3
	debug_ffb_en[3]
	debug_ffb_wdata[31:0]

	4
	—
	EBREAK


Word 4 cannot be written by the debugger and always holds EBREAK, so execution returns to debug mode at the end of the program buffer. While the program buffer is executed, all fault, error and replay status is forced to zero. A debug reset while the thread is halted rewrites words 0 to 4 with EBREAK.
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